Components writing messages to the LBR Implement interface SerialWriter

Network manager behavior:

1. Initialize GUI, start up window should be the control panel
2. Probe serial connections for list of ports
3. If only one serial device detected, print the serial port on the console and open a connection
4. If no serial devices connected say so
5. If multiple serial devices connected, do nothing but print list of devices to use as wsn LBR.